District of Columbia Municipal Regulations


SECTION 12 NORMATIVE REFERENCES
Under heading “ASHRAE” in Section 12 of ASHRAE 90.1, strike reference to “ANSI/ASHRAE Standard 62.1-2007Ventilation for Acceptable Indoor Air Quality” and insert a new standard in its place in the Energy Conservation Code-Commercial Provisions to read as follows:

Reference
Title

ASHRAE
1791 Tullie Circle, NE, Atlanta, GA 30329

ANSI/ASHRAE Standard 62.1-2013



Ventilation for Acceptable Indoor Air 
Quality

Under heading “ASHRAE” in Section 12 of ASHRAE 90.1, insert a new reference in the Energy Conservation Code-Commercial Provisions to “ANSI/ASHRAE Standard 189.1-2014” to read as follows:
ASHRAE
1791 Tullie Circle, NE, Atlanta, GA 30329

ANSI/ASHRAE Standard 189.1-2014


Standard for the Design of High-Performance Green Buildings Except 






Low-Rise Residential Buildings
Under heading “ASTM International” in Section 12 of ASHRAE 90.1, insert new references in the Energy Conservation Code-Commercial Provisions to read as follows:
ASTM International

100 Barr Harbor Dr., West Conshohocken, PA 19428-2959
ASTM E1827-11
Standard Test Methods for Determining Airtightness of Buildings Using an Orifice Blower Door

ASTM E2813-12 




     Standard Practice for Building Enclosure Commissioning

Under heading “Canadian General Standards Board” in Section 12 of ASHRAE 90.1, insert new references in the Energy Conservation Code-Commercial Provisions to read as follows:
Canadian General Standards Board (CGSB)

Place du Portage III, 6B1, 11 Laurier Street, Gatineau, Quebec, K1A 1G6 Canada

CAN/CGSB-149.10-M86
Determination of the Airtightness of Building Envelopes by the Fan Depressurization Method

CAN/CGSB 149.15-96
Determination of the Overall Envelope Airtightness of Buildings by the Fan Pressurization Method Using the Building’s Air Handling Systems

Under heading “United States Department of Energy” in Section 12 of ASHRAE 90.1, insert a new reference in the Energy Conservation Code-Commercial Provisions to read as follows:
United States Department of Energy

Office of Energy Efficiency & Renewable Energy, 1000 Independence Ave., SW, Washington, DC 20585

ENERGY STAR Multifamily Midrise T&V Protocols, 8.1
     Fan Pressure Testing; Sampling 

Requirements

SOURCE: Final Rulemaking published at 67 DCR 6326 (May 29, 2020 – Part 2).
The District of Columbia Energy Conservation Code (2017), referred to as the “Energy Conservation Code,” consists of  ANSI/ASHRAE/IES 90.1-2013, Energy Standard for Buildings Except Low-Rise Residential Buildings (ASHRAE 90.1) and substantial portions of Chapter 7 of ANSI/ASHREA/IES 189.1-2014, Standard for the Design of High-Performance Green Buildings Except Low-Rise Residential Buildings (ASHRAE 189.1), published by the American Society of Heating, Refrigeration and Air-Conditioning Engineers (ASHRAE), and the  Residential Provisions of the 2015 edition of the International Energy Conservation Code (International Energy Conservation Code), published by the International Code Council (ICC), as amended by the Energy Conservation Code Supplement of 2017 – Commercial Provisions (12-I[CE] DCMR) and the Energy Conservation Code Supplement of 2017 – Residential Provisions (12-I[RE] DCMR). The International Energy Conservation Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: https://codes.iccsafe.org/public/document/IECC2015.  ASHRAE 90.1 is copyrighted by ASHRAE and therefore is not republished here.  However, the text of ASHRAE 90.1 may be reviewed at: https://www.ashrae.org/standards-research--technology. Portions of Chapter 7 of ASHRAE 189.1 are reprinted in the District of Columbia Energy Conservation Code Supplement by permission of ASHRAE and ICC.
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