District of Columbia Municipal Regulations


913
FIRE PUMPS

Insert a new Exception 3 into Section 913.2.1 of the Fire Code to read as follows:

3. Access to the fire pump room shall not be required to be directly from the exterior or from a fire rated enclosure.

SOURCE: Final Rulemaking published at 67 DCR 6232 (May 29, 2020 – Part 2).

The District of Columbia Fire Code (2017), referred to as the “Fire Code,” consists of the 2015 edition of the International Fire Code (International Fire Code), published by the International Code Council (ICC), as amended by the Fire Code Supplement of 2017 (12-H DCMR). The International Fire Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be reviewed at:

https://codes.iccsafe.org/public/document/IFC2015.
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