District of Columbia Municipal Regulations


1405
INSTALLATION OF WALL COVERINGS

Amend Table 1405.2, MINIMUM THICKNESS OF WEATHER COVERINGS, of the International Building Code to strike the entry for “Precast stone facing”in its entirety, and revise the entry for “Minimum Thickness” of “Porcelain Tile” to read as follows:

TABLE 1405.2
MINIMUM THICKNESS OF WEATHER COVERINGS

	Covering Type
	Minimum Thickness (inches)

	Porcelain tile
	0.25


SOURCE: Final Rulemaking published at 65 DCR 6838 (June 22, 2018).
The District of Columbia Building Code (2013), referred to as the “Building Code,” consists of the 2012 edition of the International Building Code as amended by the District of Columbia Building Code Supplement (2013)(12  DCMR A). The International Building Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/ibc/2012/index.htm?bu=IC-P-2012-000001&bu2=IC-P-2012-000019.
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