District of Columbia Municipal Regulations


406
BUILDING SITE WASTE MANAGEMENT

Strike Section 406.1 of the International Green Construction Code in its entirety and insert new Section 406.1 in the Green Construction Code in its place to read as follows:
406.1 Building site waste management requirements.  Not less than 75 percent of the land-clearing debris from a building site shall be diverted from landfills. Land-clearing debris includes rock, trees, stumps and associated vegetation. The building site development shall comply with the following additional requirements:

1. The effective destruction and disposal of invasive plant species.
2. Where the site is located in a federal or state designated quarantine zone for invasive insect species, building site vegetation management shall comply with the quarantine rules.

3. Receipts or other documentation related to diversion shall be maintained through the course of construction.  When requested by the code official, evidence of diversion shall be provided.

Insert a new Section 406.3 in the Green Construction Code to read as follows:

406.3 Verification.  Prior to issuance of the first certificate of occupancy for occupiable space in a story above grade plane, or prior to final inspection, if a new certificate of occupancy is not required, the Department is authorized to require the owner, contractor or an approved agency to provide verification of the project’s compliance with Section 406.1. 
SOURCE: Final Rulemaking published at 67 DCR 6509 (May 29, 2020 – Part 2).
The District of Columbia Green Construction Code (2017), referred to as the “Green Construction Code,” consists of the 2012 edition of the International Green Construction Code (International Green Construction Code), published by the International Code Council (ICC), as amended by the District of Columbia Green Construction Code Supplement  of 2017 (12-K DCMR). The International Green Construction Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at:
https://codes.iccsafe.org/public/document/toc/548/.
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