District of Columbia Municipal Regulations


801
GENERAL

Strike Section 801.18 of the International Mechanical Code and insert a new Section 801.18 into the Mechanical Code to read as follows:

801.18 Existing chimneys and vents. Where an appliance is permanently disconnected from an existing chimney or vent, or where an appliance is connected to an existing chimney or vent during the process of a new installation, the chimney or vent shall comply with Sections 801.18.1 through 801.18.4. Where a new or replacement vented appliance is approved for use in connection with an existing chimney not currently in use, compliance with Section 801.18.5 is required.

[No change to Sections 801.18.1 through 801.18.4 of the International Mechanical Code]

Insert a new Section 801.18.5 into the Mechanical Code to read as follows:

801.18.5 Integrity inspection.  Before a new or replacement vented appliance is approved for use in connection with an existing chimney not currently in use, the chimney shall be relined or shall be inspected for integrity by the permit holder in the presence of the code official, using a scented smoke test or other approved method.  In lieu of observing the test, the code official is authorized to accept a certification of integrity of the chimney, issued by the D.C.-licensed contractor who conducted the inspection or test.

SOURCE: Final Rulemaking published at 67 DCR 6078 (May 29, 2020 – Part 2).
The District of Columbia Mechanical Code (2017), referred to as the “Mechanical Code,” consists of the 2015 edition of the International Mechanical Code (International Mechanical Code), published by the International Code Council (ICC), as amended by the Mechanical Code Supplement of 2017 (12-E DCMR). The International Mechanical Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: https://codes.iccsafe.org/public/document/toc/549.
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