District of Columbia Municipal Regulations


3501


Amend Chapter 35, REFERENCED STANDARDS, of the Building Code to read as follows:

Strike the Standard Reference Number ASTM/E 84-09 and insert the new Standard Reference Number ASTM/E 84-2013A in its place, and add code references 1403.5 and 2603.5.5 to this entry; and further, strike the Standard Reference Number ASTM/E 1354-09 and insert the new Standard Reference Number ASTM/E 1354-2013 in its place, and add code reference 1403.5 to this entry, to read as follows: 
	ASTM
	ASTM International 
100 Barr Harbor Drive 
West Conshohocken, PA 19428-2959
	

	Standard Reference Number
	Title
	Referenced in code section number

	E84-2013A

	Test Methods for Surface Burning Characteristics of Building Materials. 
	202, 402.6.4.4, 406.7.2,

703.5.2, 720.1, 720.4, 803.1.1, 803.1.4, 803.9, 803.13, 806.5, 1404.12.1, 1407.9,

1407.10.1, 1409.9, 1409.10.1, 1509.6.2, 1509.6.3, 2303.2, 2603.3,

2603.4.1.13, 2603.7, 2604.2.4, 2606.3.5.4, 2606.4, 2613.3, 3105.3, 1403.5,

2603.5.5



	E1354-2013


	Standard Test Method for Heat and Visible Smoke Release Rates for 

Materials and Products Using an Oxygen Consumption Calorimeter
	424.2, 1403.5


SOURCE: Final Rulemaking published at 61 DCR 2782 (March 28, 2014 – Part 2); as amended by Final Rulemaking published at 65 DCR 6838 (June 22, 2018). 

The District of Columbia Building Code (2013), referred to as the “Building Code,” consists of the 2012 edition of the International Building Code as amended by the District of Columbia Building Code Supplement (2013)(12  DCMR A). The International Building Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/ibc/2012/index.htm?bu=IC-P-2012-000001&bu2=IC-P-2012-000019.
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