District of Columbia Municipal Regulations


802
INDIRECT WASTES

Strike Section 802.3 of the International Plumbing Code in its entirety and insert a new Section 802.3 into the Plumbing Code in its place to read as follows:

802.3 Waste receptors. Waste receptors shall be of an approved type. A removable strainer or basket shall cover the waste outlet of all waste receptors. Waste receptors shall be installed in ventilated spaces. Waste receptors shall not be installed in bathrooms, toilet rooms, plenums, crawl spaces, attics, interstitial spaces above ceilings and below floors or in any inaccessible or unventilated space such as a closet or storeroom. Ready access shall be provided to waste receptors.

Exception: Clothes washer standpipes shall be permitted in bathrooms in dwelling units.
SOURCE: Final Rulemaking published at 67 DCR 6148 (May 29, 2020 – Part 2).
The District of Columbia Plumbing Code (2017), referred to as the “Plumbing Code,” consists of the 2015 edition of the International Plumbing Code (International Plumbing Code), published by the International Code Council (ICC), as amended by the Plumbing Code Supplement of 2017 (12-F DCMR). The International Plumbing Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: https://codes.iccsafe.org/public/document/IPC2015.
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