District of Columbia Municipal Regulations


4905

REAR YARD

4905.1
A rear yard shall be provided for each public school, the minimum depth of which shall be as set forth in the following table:

TABLE K § 4905.1:  MINIMUM REAR YARD FOR PUBLIC SCHOOLS

	Zone
	Minimum Rear Yard

	RC-1
	4 in./ft. of vertical distance from the mean finished grade at the middle of the rear of the structure to the highest point of the main roof or parapet wall, but not less than 15 ft.

	RC-2, RC-3
	As permitted by zone


4905.2 
In the case of a lot proposed to be used by a public school that abuts or adjoins along the rear lot line a public open space, recreation area, or reservation, no rear yard shall be required.

SOURCE: Final Rulemaking published at 67 DCR 3776 (April 3, 2020).
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