District of Columbia Municipal Regulations


402
FACILITY MAINTENANCE ─ REFUSE AND REMOVAL FREQUENCY
402.1
Inside and outside receptacles shall be of sufficient capacity to hold all accumulated refuse.   

402.2
Refuse discarded indoor shall be in a lined waste receptacle at a frequency that does not create a nuisance.

402.3
Receptacles and waste handling units shall be constructed of:

(a)
Durable material that is rodent-resistant, leak-proof, nonabsorbent, and easily cleanable; 

(b)
Designed with tight-fitting lids, doors, or covers;

(c)
Maintained in good repair.

402.4
If used, an outdoor enclosure for refuse shall be constructed of durable and cleanable materials and shall be located so that a public health hazard or nuisance is not created.

402.5
An outdoor storage surface for refuse shall be constructed of nonabsorbent material such as concrete or asphalt and shall be smooth, durable, and sloped to drain.  

402.6
Storage areas and enclosures for refuse shall be kept clean and maintained free of unnecessary items and in good repair.

SOURCE: Final Rulemaking published at 68 DCR 013026 (December 10, 2021).
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