District of Columbia Municipal Regulations


206

FRONT SETBACK 

206.1
Except as provided elsewhere in this title, the front setback requirements shall be as set forth in this section.

206.2
For all detached residential buildings, a front setback shall be provided within the range of existing front setbacks of all residential buildings on the same side of the street in the block where the building is proposed.
206.3
For an interior-lot row or semi-detached building, a front setback shall be provided that is no further forward or further back than the building façade of one (1) of the immediately adjoining buildings.

SOURCE: Final Rulemaking published at 63 DCR 2447, 2887 (March 4, 2016 – Part 2); as amended by Final Rulemaking published at 63 DCR 10620 (August 19, 2016); as amended by Final Rulemaking published at 64 DCR 4055 (April 28, 2017); as amended by Final Rulemaking published at 64 DCR 8596 (September 1, 2017); as amended by Final Rulemaking published at 67 DCR 13346 (November 13, 2020); as amended by Errata Notice published at 68 DCR 405 (January 8, 2021); as amended by Final Rulemaking published at 68 DCR 013834 (December 24, 2021); as amended by Final Rulemaking published at 70 DCR 011297 (August 25, 2023); as amended by Final Rulemaking published at 73 DCR 009999 (July 10, 2026).
	
	Zoning Regulations of 2016: 
Residential Flat (RF) Zones
11-E DCMR § 206

	

	
	
	



