District of Columbia Municipal Regulations


922
KEROSENE AND OIL-FIRED STOVES

Strike Section 922.1 of the International Mechanical Code in its entirety and insert a new Section 922.1 into the Mechanical Code in its place to read as follows:

922.1 General.  Kerosene and oil-fired stoves shall not be used or installed in any premises. 

SOURCE: Final Rulemaking published at 67 DCR 6078 (May 29, 2020 – Part 2).
The District of Columbia Mechanical Code (2017), referred to as the “Mechanical Code,” consists of the 2015 edition of the International Mechanical Code (International Mechanical Code), published by the International Code Council (ICC), as amended by the Mechanical Code Supplement of 2017 (12-E DCMR). The International Mechanical Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: https://codes.iccsafe.org/public/document/toc/549.
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