District of Columbia Municipal Regulations


604

ELECTRICAL FACILITIES

Strike Section 604.2 of the International Property Maintenance Code in its entirety and insert new Section 604.2 in the Property Maintenance Code in its place to read as follows:

604.2 Service.  The size and usage of appliances and equipment shall serve as a basis for determining the need for additional facilities in accordance with NFPA 70.  Dwelling units shall be served by a three-wire, 120/240 volt, single-phase electrical service having a rating of not less than 60 amperes.

Exception:  For installations consisting of not more than two 2-wire branch circuits, service disconnecting means shall have a rating of not less than 30 amperes.

SOURCE: Final Rulemaking published at 67 DCR 6173 (May 29, 2020 – Part 2).
The District of Columbia Property Maintenance Code (2017), referred to as the “Property Maintenance Code,” consists of the 2015 edition of the International Property Maintenance Code (International Property Maintenance Code), published by the International Code Council (ICC), as amended by the Property Maintenance Code Supplement of 2017 (12-G DCMR). The International Property Maintenance Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at:
https://codes.iccsafe.org/public/document/toc/551/
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