District of Columbia Municipal Regulations


314
CONDENSATE DISPOSAL

Strike Section 314.2.1 of the International Plumbing Code in its entirety and substitute a new Section 314.2.1 into the Plumbing Code in its place to read as follows:

314.2.1 Condensate disposal.  Condensate from all cooling coils and evaporators shall be conveyed from the drain pan outlet to an approved place of disposal.  Such piping shall maintain a horizontal slope in the direction of discharge of not less than one-eighth unit vertical in 12 units horizontal (1-percent slope).  Condensate shall not discharge into a street, alley or other areas so as to cause a nuisance.  Condensate shall not discharge into separate sanitary sewer systems.  

Exception: In the replacement in-kind of existing equipment, condensate disposal shall be allowed to use the existing discharge piping system.

SOURCE: Final Rulemaking published at 67 DCR 6148 (May 29, 2020 – Part 2).
The District of Columbia Plumbing Code (2017), referred to as the “Plumbing Code,” consists of the 2015 edition of the International Plumbing Code (International Plumbing Code), published by the International Code Council (ICC), as amended by the Plumbing Code Supplement of 2017 (12-F DCMR). The International Plumbing Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: https://codes.iccsafe.org/public/document/IPC2015.
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