District of Columbia Municipal Regulations


M1502 
CLOTHES DRYER EXHAUST

Strike Section M1502.4.2 of the International Residential Code in its entirety and insert a new Section M1502.4.2 into the Residential Code in its place to read as follows:

M1502.4.2 Duct installation.  Exhaust ducts shall be supported at intervals not to exceed 4 feet (1219 mm) and shall be secured in place.  The insert end of the duct shall extend into the adjoining duct or fitting in the direction of airflow.  Exhaust duct joints shall be sealed in accordance with Section M1601.4.1 and shall be mechanically fastened.  Ducts shall not be joined with screws or similar fasteners that protrude more than 1/8 inch (3.2 mm) into the inside of the duct.

SOURCE: Final Rulemaking published at 67 DCR 6033 (May 29, 2020 – Part 2).
The District of Columbia Residential Code (2017), referred to as the “Residential Code,” consists of the 2015 edition of the International Residential Code (International Residential Code), published by the International Code Council (ICC), as amended by the Residential Code Supplement of 2017 (12-B DCMR). The International Residential Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at https://codes.iccsafe.org/public/document/IRC2015.
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