District of Columbia Municipal Regulations


406
DECKS AND DECK EQUIPMENT

Strike Section 406.2 of the International Swimming Pool and Spa Code in its entirety and substitute a new Section 406.2 of the Swimming Pool and Spa Code in its place, to read as follows:

406.2 Pool perimeter access.  A deck or unobstructed access shall be provided for not less than 90 percent of the pool perimeter.  For the purpose of this section, the length of the infinity edge of a Class C infinity swimming pool shall not be counted towards the perimeter of the pool.
SOURCE: Final Rulemaking published at 67 DCR 6587 (May 29, 2020 – Part 2).

The District of Columbia Swimming Pool and Spa Code (2017), referred to as the “Swimming Pool and Spa Code,” consists of the 2015 edition of the International Swimming Pool and Spa Code (International Swimming Pool and Spa Code), published by the International Code Council (ICC), as amended by the Swimming Pool and Spa Code Supplement of 2017 (12-L DCMR). The International Swimming Pool and Spa Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at:
https://codes.iccsafe.org/public/document/toc/555.                
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