District of Columbia Municipal Regulations


705  
SIDE YARD (RC)

705.1 A minimum side yard shall be provided for each structure located in the RC zones as set forth in the following table:

TABLE K § 705.1:  MINIMUM SIDE YARD

	Zone
	Minimum Side Yard Distance

	RC-1
	None required; however, if a side yard is provided, it shall be no less than 4 ft.

	RC-2
	None required for a principal building; however, if a side yard is provided, it shall be at least 2 in. wide for each 1 ft. of height of building but no less than 5 ft.

	RC-3
	None required for a principal building; however, if a side yard is provided, it shall be at least 2 in. wide for each 1 ft.  of height of building but no less than 5 ft.


705.2 In the RC-2 and RC-3 zones, any portion of a building setback from the side lot line shall be considered a side yard and not a court.

SOURCE: Final Rulemaking published at 63 DCR 2447, 3176 (March 4, 2016 – Part 2).
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