District of Columbia Municipal Regulations


1003
GENERAL MEANS OF EGRESS

Strike Section 1003.2 of the International Building Code in its entirety and insert new Section 1003.2 in the Building Code in its place to read as follows:

1003.2 
Ceiling height.  The means of egress shall have a ceiling height of not less than 7 feet (2134 mm).

Exceptions:

1. Sloped ceilings in accordance with Section 1208.2.

2. Ceilings of dwelling units and sleeping units within residential occupancies in accordance with Section 1208.2.

3. Allowable projections in accordance with Section 1003.3.

4. Stair headroom in accordance with Section 1009.5.

5. Door height in accordance with Section 1008.1.1.

6. Ramp headroom in accordance with Section 1010.6.2.

SOURCE: Final Rulemaking published at 61 DCR 2782 (March 28, 2014 – Part 2).
The District of Columbia Building Code (2013), referred to as the “Building Code,” consists of the 2012 edition of the International Building Code as amended by the District of Columbia Building Code Supplement (2013)(12  DCMR A). The International Building Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/ibc/2012/index.htm?bu=IC-P-2012-000001&bu2=IC-P-2012-000019.
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