District of Columbia Municipal Regulations


803
HVAC SYSTEMS

Strike Section 803.2 of the International Green Construction Code in its entirety without substitution. 

Strike Section 803.3 of the International Green Construction Code in its entirety without substitution.

Strike Section 803.4 of the International Green Construction Code in its entirety without substitution.

Strike Section 803.5 of the International Green Construction Code in its entirety and insert new Section 803.5 in the Green Construction Code to read as follows: 

803.5 
Filters.  Filters for air conditioning systems that serve occupied spaces and handle a component of outdoor air shall be rated at MERV 11 or higher, in accordance with ASHRAE Standard 52.2, and system equipment shall be designed to be compatible.  The air handling system design shall account for pressure drop across the filter.  Filter performance shall be shown on the filter manufacturer’s data sheet.

SOURCE: Final Rulemaking published at 61 DCR 3356 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Green Construction Code (2013) , referred to as the “Green Construction Code,” consists of the 2012 edition of the International Green Construction Code published by the International Code Council (ICC), as amended by the District of Columbia Green Construction Code Supplement (2013)(12 DCMR K).  The International Green Construction Code is copyrighted by the International Code Council and therefore is not republished here.  However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/igcc/2012/index.htm?bu=IC-P-2012-000023&bu2=IC-P-2012-000019. 
	
	Green Construction Code Supplement of 2013
12-K DCMR § 803

	

	
	
	



