District of Columbia Municipal Regulations


802
BUILDING CONSTRUCTION FEATURES, OPERATIONS AND MAINTENANCE FACILITATION

Strike Section 802.3 of the International Green Construction Code in its entirety and insert new Section 802.3 in the Green Construction Code in its place to read as follows:
802.3 
Air-handling system filters.  Filter racks shall be designed to prevent airflow from bypassing filters.  Access doors and panels provided for filter replacement shall be fitted with flexible seals to provide an effective seal between the doors and panels and the mating filter rack surfaces.  Filter access panels and doors shall not be obstructed.
SOURCE: Final Rulemaking published at 61 DCR 3356 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Green Construction Code (2013) , referred to as the “Green Construction Code,” consists of the 2012 edition of the International Green Construction Code published by the International Code Council (ICC), as amended by the District of Columbia Green Construction Code Supplement (2013)(12 DCMR K).  The International Green Construction Code is copyrighted by the International Code Council and therefore is not republished here.  However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/igcc/2012/index.htm?bu=IC-P-2012-000023&bu2=IC-P-2012-000019. 
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