1311
HIGH DENSITY USE OF BATHROOM FACILITIES

1311.1
Notwithstanding the requirements of § 602 of this subtitle, hotels or motels which have high-density occupancy of any sleeping rooms, as permitted under the provisions of this chapter, may permit not more than ten (10) transients to use one water closet, one lavatory, and one bathing facility in order to accommodate the additional occupants allowed by this chapter.

1311.2
Any transient accommodated in a room not provided with a bathroom containing a water closet, lavatory, and bathing facility shall have those facilities available for his or her use in a hall bathroom.

1311.3
Each hall bathroom shall be on the same floor with the sleeping accommodations it is intended to serve.


SOURCE: The Housing Regulations of the District of Columbia, 5G DCRR § 7303, Commissioners’ Order 53-1503 (August 11, 1955); as amended by Commissioners’ Order 63-1354 (June 6, 1963), 9 DCR 276 (June 4, 1963).

