District of Columbia Municipal Regulations


1203
VENTILATION

Strike Section 1203.1 of the International Building Code in its entirety and insert new Section 1203.1 in the Building Code in its place to read as follows:

1203.1 
General.  Buildings shall be provided with natural ventilation in accordance with Section 1203.4, or mechanical ventilation in accordance with the Mechanical Code.  Each new dwelling unit shall be ventilated by mechanical means in accordance with Section 403 of the Mechanical Code and shall have at least one opening to the outdoors for natural ventilation of not less than 4 percent of the floor area of the habitable spaces of the dwelling unit.

SOURCE: Final Rulemaking published at 61 DCR 2782 (March 28, 2014 – Part 2).
The District of Columbia Building Code (2013), referred to as the “Building Code,” consists of the 2012 edition of the International Building Code as amended by the District of Columbia Building Code Supplement (2013)(12  DCMR A). The International Building Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/ibc/2012/index.htm?bu=IC-P-2012-000001&bu2=IC-P-2012-000019.
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