District of Columbia Municipal Regulations


922
KEROSENE AND OIL-FIRED STOVES

Strike Section 922.1 of the International Mechanical Code in its entirety and insert new Section 922.1 in the Mechanical Code in its place to read as follows:

922.1 
General.  Kerosene and oil-fired stoves shall not be used or installed in any premises.
SOURCE: Final Rulemaking published at 61 DCR 3101 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Mechanical Code (2013), referred to as the “Mechanical Code,” consists of the 2012 edition of the International Mechanical Code, published by the International Code Council (ICC), as amended by the District of Columbia Mechanical Code Supplement (2013)(12 DCMR E). The International Mechanical Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/imc/2012/index.htm?bu=IC-P-2012-000005&bu2=IC-P-2012-000019.
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