District of Columbia Municipal Regulations


107 
MAINTENANCE

Strike Chapter 1 of the International Fire Code in its entirety and insert new Chapter 1 in the Fire Code in its place to read as follows:
107.1 
Maintenance of Safeguards.  Whenever or wherever any device, equipment, system, condition, arrangement, level of protection, or any other feature is required for compliance with the provisions of the Fire Code, or otherwise installed, such device, equipment, system, condition, arrangement, level of protection, or other feature shall thereafter be continuously maintained in accordance with the Fire Code and applicable referenced standards.

107.2 
Testing and Operation.  Equipment requiring periodic testing or operation to ensure maintenance shall be tested or operated as specified in the Fire Code.

107.2.1 Test and Inspection Records.  Required test and inspection records shall be available to the code official at all times, and such records as designated shall be filed with the code official.

107.2.2 Reinspection and Testing.  Where any work or installation does not pass an initial test or inspection, the necessary corrections shall be made so as to achieve compliance with the Fire Code.  The work or installation shall then be resubmitted to the code official for inspection and testing.

107.3 
Supervision.  Maintenance and testing shall be under the supervision of a responsible person who shall ensure that such maintenance and testing is conducted at specified intervals in accordance with the Fire Code.

107.4 
Rendering Equipment Inoperable.  Portable or fixed fire-extinguishing systems or devices and fire-warning systems shall not be rendered inoperative or inaccessible except as necessary during emergencies, maintenance, repairs, alterations, drills or prescribed testing.

107.5 
Overcrowding.  Overcrowding or admittance of any person beyond the approved capacity of a building or a portion thereof shall not be allowed.  The code official, upon finding any overcrowding conditions or obstructions in aisles, passageways or other means of egress, or upon finding any condition which constitutes a life safety hazard, shall be authorized to cause the event to be stopped until such condition or obstruction is corrected.

SOURCE: Final Rulemaking published at 61 DCR 3251 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Fire Code (2013), referred to as the “Fire Code,” consists of the 2012 edition of the International Fire Code  as amended by the District of Columbia Fire Code Supplement (2013) (12 DCMR H).  The International Fire Code is copyrighted by the International Code Council and therefore is not republished here.  However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/ifc/2012/index.htm?bu=IC-P-2012-000003&bu2=IC-P-2012-000019.
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