606
CLEANABILITY ─ FLOOR AND WALL JUNCTURES, COVERED, AND ENCLOSED OR SEALED  

606.1
Floor and wall junctures shall be covered and closed to no larger than one millimeter (1 mm.) or one thirty-second of an inch (1/32 in.). 
606.2
Covering of floor and wall junctures shall be sealed.  

SOURCE: Final Rulemaking published at 60 DCR 3582 (March 15, 2013).
