607
CLEANABILITY ─ FLOOR CARPETING, RESTRICTIONS AND INSTALLATION  

607.1
A floor covering such as carpeting or similar material shall not be installed as a floor covering in toilet room areas where handwashing sinks, toilets, or urinals are located; refuse storage rooms; or other areas where the floor is subject to moisture. 

607.2
If carpeting is installed as a floor covering in areas other than those specified in Section 607.1, it shall be:  

(a)
Securely attached to the floor with a durable mastic, by using a stretch and 
tack method, or by another similar method; and

(b)
Installed tightly against the wall under the coving or installed away from 
the wall with a space between the carpet and the wall and with the edges 
of the carpet secured by metal stripping or some other means.  

SOURCE: Final Rulemaking published at 60 DCR 3582 (March 15, 2013).
