District of Columbia Municipal Regulations


604
EMERGENCY AND STANDBY POWER SYSTEMS

Strike Section 604.5.1 of the International Fire Code in its entirety and insert new Section 604.5.1 in its place in the Fire Code to read as follows:

604.5.1. Activation test.  An activation test of the emergency lighting equipment shall be completed annually. The activation test shall ensure the emergency lighting activates automatically upon normal electrical disconnect and stays sufficiently illuminated for a minimum of 30 seconds.


(No change to Section 604.5.1.1 of the International Fire Code.) 

SOURCE: Final Rulemaking published at 61 DCR 3251 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Fire Code (2013), referred to as the “Fire Code,” consists of the 2012 edition of the International Fire Code  as amended by the District of Columbia Fire Code Supplement (2013) (12 DCMR H).  The International Fire Code is copyrighted by the International Code Council and therefore is not republished here.  However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/ifc/2012/index.htm?bu=IC-P-2012-000003&bu2=IC-P-2012-000019.
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