District of Columbia Municipal Regulations


402  
DENSITY – FLOOR AREA RATIO (FAR) (HE)

402.1 The maximum permitted FAR of buildings in HE zones shall be given in the following table:

TABLE K § 402.1:  MAXIMUM PERMITTED FAR

	HE Sub-district
	Maximum FAR

	HE-1 (19th St.)
	3.0

	HE-2 (20th St.)
	4.8

	HE-3 (Water St.)
	7.2

	HE-4 (Corrections)
	6.0

	Square  E (Park)
	0.2


402.2 The following density limitations on non-residential uses apply within the HE zones, but only in the squares listed below:

TABLE K § 402.2:  MAXIMUM FAR FOR NON-RESIDENTIAL USES

	Square
	Maximum Non-residential FAR

	F
	0.8

	G
	1.0

	H
	0.5

	I
	3.0


402.3 The matter-of-right FAR shall serve as the maximum permitted height and floor area ratio for a planned unit development (PUD).

402.4 The minimum lot area for row dwellings shall be eighteen hundred square feet (1,800 sq. ft.) with a minimum lot width of eighteen feet (18 ft.).

SOURCE: Final Rulemaking published at 63 DCR 2447, 3176 (March 4, 2016 – Part 2).
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