District of Columbia Municipal Regulations


316
FRONT BUILD-TO LINES
316.1
When a zone has a front build-to requirement, the front façade of all buildings and structures must directly abut the build-to line.
SOURCE: Final Rulemaking published at 63 DCR 2447, 2650 (March 4, 2016 – Part 2).
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