District of Columbia Municipal Regulations


905  
SIZE AND LAYOUT REQUIREMENTS

905.1 The intent of this section is to ensure that loading facilities are adequately sized and capable of performing their intended functions.

905.2 All loading berths shall be a minimum of twelve feet (12 ft.) wide, have a minimum depth of thirty feet (30 ft.) and have a minimum vertical clearance of fourteen feet (14 ft.).

905.3 All service/delivery spaces shall be a minimum of ten feet (10 ft.) wide, have a minimum depth of twenty feet (20 ft.), and have a minimum vertical clearance of ten feet (10 ft.). 

905.4 All loading berths shall be accompanied by one (1) adjacent loading platform that meets the following requirements:

(a) A loading berth that is less than fifty-five feet (55 ft.) deep shall have a platform that is at least one hundred square feet (100 sq. ft.) and at least eight feet (8 ft.) wide;

(b) A loading berth that is fifty-five feet (55 ft.) deep or greater shall have a platform that is at least two hundred square feet (200 sq. ft.) and at least twelve feet (12 ft.) wide;

(c) Loading platforms shall have a minimum vertical clearance of ten feet (10 ft.); and

(d) A loading platform floor shall consist of one (1) horizontal level.

905.5 No loading platform need be provided for loading berths if the required loading berth is increased in depth for the full width thereof, such that the resulting enlarged loading berth is equal in area to the combined area of a required loading berth and a required loading platform.

905.6 The dimensions specified in this section for loading berths and service/delivery spaces are exclusive of access aisles, maneuvering space, and loading platforms.

SOURCE: Final Rulemaking published at 63 DCR 2447, 2712 (March 4, 2016 – Part 2).
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