District of Columbia Municipal Regulations


3500


Strike Standard Reference Numbers ASME/A17.1 2007/CSA B44-07, A18.1—2008, A90.1—09, and B20.1—2009 under subheading ASME in Chapter 35 Referenced Standards of the International Building Code in their entirety and insert new Standard Reference Numbers ASME/A17.1 2010/CSA B44-10,  A18.1—2008, A90.1—09, and B20.1—2009 under subheading ASME  in Chapter 35 Referenced Standards of the Building Code in their place to read as follows:
	ASME
	American Society of Mechanical Engineers
Three Park Avenue
New York, NY 10016-5990
	

	Standard Reference Number
	Title
	Referenced in code section number

	ASME/A17.1 2010/CSA B44-10
	Safety Code for Elevators and Escalators
	907.3.3, 911.1.5, 1007.4, 1607.9.1, 3001.2, 3001.4, 3002.5, 3003.2, 3007.1, 3007.2, 3008.2, 3008.2.1, 3008.7.6, 3008.8.1, 3009.1,3010.2.2.1, 3010.5.4.1

	A18.1—2008 
	Safety Standard for Platform Lifts and Stairway Chairlifts 
	1109.8 , 2702.2.6 ,3001.2, 3010.5.2 

	A90.1—2009 
	Safety Standard for Belt Manlifts 
	3001.2, 3010.5.3 

	B20.1—2009 
	Safety Standard for Conveyors and Related Equipment 
	3001.2, 3005.3, 3010.5.4,  


SOURCE: Final Rulemaking published at 61 DCR 2782 (March 28, 2014 – Part 2).
The District of Columbia Building Code (2013), referred to as the “Building Code,” consists of the 2012 edition of the International Building Code as amended by the District of Columbia Building Code Supplement (2013)(12  DCMR A). The International Building Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/ibc/2012/index.htm?bu=IC-P-2012-000001&bu2=IC-P-2012-000019.
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