District of Columbia Municipal Regulations


405 
INSTALLATION OF FIXTURES
Strike Section 405.3.2 of the International Plumbing Code in its entirety and insert new Section 405.3.2 in the Plumbing Code in its place to read as follows:

405.3.2 Public lavatories.  Lavatories shall be installed within multiple-occupancy employee and public toilet rooms that contain one or more water closets or urinals.  The number of such lavatories shall be sufficient to serve the occupant load served by the water closets and urinals located in the same toilet room, based on the ratios of Table 403.1.  All single-occupancy employee and public toilet rooms shall contain a lavatory.  Lavatories installed outside a toilet room shall not count towards the number of lavatories required by Table 403.1 for employee and public toilet facilities.

SOURCE: Final Rulemaking published at 61 DCR 3169 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Plumbing Code (2013), referred to as the “Plumbing Code,” consists of the 2012 edition of the International Plumbing Code  as amended by the District of Columbia Plumbing Code Supplement (2013) (12 DCMR F). The International Plumbing Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/ipc/2012/index.htm?bu=IC-P-2012-000004&bu2=IC-P-2012-000019.
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