603
WATERPROOF FLOORS IN TOILETS

603.1
The owner of a building used for residential purposes shall provide each water closet compartment, privy, toilet room, and bathroom in the building with a waterproof floor surface and wall base.

603.2
The wall base shall be at least three inches (3”) in height.

603.3
The waterproof floor surface shall consist of one of the following:

(a)
Smooth-finished tile or masonry which is effectively sealed so that it has a nonporous surface, laid in a manner free from cracks or open joints, and tightly joined to the base;

(b)
Tongue-and-groove hardwood flooring that is tightly laid without open cracks or joints, and which is tightly joined to the base. Both the base and surface shall be covered with a seal coat of waterproof finish; or

(c)
Linoleum, plastic, or rubber floor covering, or linoleum, asphalt, rubber or plastic floor tiles, firmly cemented to a smooth substantial subfloor, laid without overlapping or open joints, and tightly joined to the base.

603.4
The term “linoleum” as used in this section, means a floor covering made of special preparations of linseed oil, gum, coloring matter, and wood flour, firmly affixed to a cloth or feltpaper base, and does not include enameled and cottonlinter composition coverings.


SOURCE: The Housing Regulations of the District of Columbia, 5G DCRR § 1202, Commissioners’ Order 55-1503 (August 11, 1955).

