403
DESIGN & CONSTRUCTION ─ TANNING STAND-UP BOOTHS, CABINETS AND VERTICAL TANNING DEVICES – ADDITIONAL REQUIREMENTS AND TEMPERATURE*

403.1
Tanning stand-up booths or cabinets or vertical tanning devices shall have physical barriers or other means compliant with 21 C.F.R. § 1040.20 (Sunlamp products and ultraviolet lamps intended for use in sunlamp products, such as floor markings, to indicate the manufacturer’s recommended exposure distance between the ultraviolet lamps and the consumer’s skin).

403.2
The temperatures inside of enclosed tanning booths or cabinets or vertical tanning devices shall be maintained below one hundred degrees Fahrenheit (100 ºF) (thirty-eight degrees Celsius (38 ºC)).

403.3
Tanning stand-up booths or cabinets or vertical tanning devices shall be constructed with sufficient strength and rigidity to withstand the stress of use and the impact of a falling person.

403.4
Access to tanning stand-up booths or cabinets or vertical tanning devices shall be of rigid construction with doors which are non-locking and open outwardly. 

403.5
Tanning stand-up booths or cabinets or vertical tanning devices shall be constructed with non-slip floors to reduce the potential for injuries from falls. 

403.6
The floor inside each tanning stand-up booth or cabinet or vertical tanning devices shall be constructed of easily cleanable surfaces and of such material, finish and so fabricated that residue may be effectively removed by normal cleaning methods. 

403.7
The floor inside each tanning stand-up booth or cabinet or vertical tanning devices shall be cleaned and sanitized as specified in Section 408, and maintained in a non-slip manner as specified in Section 403.5.

403.8
Tanning stand-up booths or cabinets or vertical tanning devices shall be maintained in good condition as specified in Section 407.

403.9
Tanning stand-up booths or cabinets or vertical tanning devices shall comply with all applicable provisions of these regulations.
SOURCE: Final Rulemaking published at 60 DCR 3582 (March 15, 2013).
