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DESIGN & CONSTRUCTION ─ TANNING EQUIPMENT AND DEVICES, AND SUPPLIES, BULBS, SHIELDING*

405.1
Each ultraviolet lamp contained within the sunlamp product shall be shielded by two (2) one-piece covers (top and bottom) without cracks or breaks in the acrylic surfaces to prevent contact with the user.
SOURCE: Final Rulemaking published at 60 DCR 3582 (March 15, 2013).
