District of Columbia Municipal Regulations


903
BUILDING ELEMENTS AND MATERIALS

Insert new Section 903.4 in the Existing Building Code to read as follows:
903.4 
Air-borne sound.  Walls, partitions and floor/ceiling assemblies separating dwelling units from each other or from public or service areas shall have a sound transmission class (STC) of not less than 50 (45 if field tested) for air-borne noise when tested in accordance with ASTM E 90. Walls, partitions and floor/ceiling assemblies separating Group A-2 occupancies from dwelling units shall have a sound transmission class (STC) of not less than 55 and shall be field tested to achieve a rating of not less than 50 for air-borne noise. Penetrations or openings in construction assemblies for piping; electrical devices; recessed cabinets; bathtubs; soffits; or heating, ventilating or exhaust ducts shall be sealed, lined, insulated or otherwise treated to maintain the required ratings. This requirement shall not apply to dwelling unit entrance doors; however, such doors shall be tight fitting to the frame and sill.

Exception: Group A-2 occupancies that do not utilize amplified music as part of their use shall be exempt from these provisions. 

SOURCE: Final Rulemaking published at 61 DCR 3336 (March 28, 2014 – Part 2).
The District of Columbia Existing Building Code (2013), referred to as the “Existing Building Code,” consists of the 2012 edition of the International Existing Building Code as amended by the District of Columbia Existing Building Code Supplement (2013)(12 DCMR J)). The International Existing Building Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/iebc/2012/index.htm?bu=IC-P-2012-000006&bu2=IC-P-2012-000019. 
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