501
DESIGN, CONSTRUCTION, AND INSTALLATION ─ APPROVED SYSTEM AND CLEANABLE FIXTURES*

501.1
Each tanning facility’s plumbing system shall be designed, constructed, and installed according to the International Plumbing Code (2006 edition), Subtitle F (Plumbing Code Supplement) of Title 12 of the District of Columbia Municipal Regulations.

501.2
Each tanning facility’s plumbing system shall be designed, constructed, installed, and maintained according to the International Plumbing Code (2006 edition), Subtitle F (Plumbing Code Supplement) of Title 12 of the District of Columbia Municipal Regulations and shall be of sufficient size to: 

(a)
Properly convey sewage and liquid disposable waste from the premises; 

(b)
Avoid creating any unsanitary condition or constituting a source of 
contamination to potable water, tanning equipment, and devices; and

(c)
Provide sufficient floor drainage to prevent excessive pooling of water or 
other disposable waste in all areas where floors are subject to flooding-
type cleaning or where normal operations release or discharge water or 
other liquid waste on the floor. 

501.3
Each plumbing fixture such as a handwashing facility, toilet, or urinal shall be easily cleanable.N  

501.4
Each tanning facility shall be equipped with effective plumbing and sewage facilities and adequate accommodations.  

SOURCE: Final Rulemaking published at 60 DCR 3582 (March 15, 2013).
