502
DESIGN, CONSTRUCTION, AND INSTALLATION ─ HANDWASHING SINKS, WATER TEMPERATURE, AND FLOW 
502.1
All handwashing sinks, including those in toilet rooms, shall be equipped to provide water at a temperature of at least one hundred degrees Fahrenheit (100 °F) (thirty-eight degrees Celsius (38 °C)) through a mixing valve, a combination faucet, or tempered water and a single faucet.

502.2
A steam mixing valve shall not be used at a handwashing sink.  

502.3
A self-closing, slow-closing, or metering faucet shall provide a flow of water for at least fifteen (15) seconds without the need to reactivate the faucet.  

502.4
Any automatic handwashing facility shall be installed in accordance with the manufacturer’s instructions.

SOURCE: Final Rulemaking published at 60 DCR 3582 (March 15, 2013).
