505
DESIGN, CONSTRUCTION AND INSTALLATION – TOILETS AND URINALS, ENCLOSED

505.1
Toilet facilities shall be provided in accordance with Section 506 and the International Plumbing Code (2006 edition), Subtitle F (Plumbing Code Supplement) of Title 12 of the District of Columbia Municipal Regulations.

505.2
A toilet room located on the premises shall be completely enclosed and provided with a tight-fitting and self-closing door, except that this requirement does not apply to a toilet room that is located outside a tanning facility. 

505.3
Toilet room doors shall be kept closed except during cleaning and maintenance operations.  

SOURCE: Final Rulemaking published at 60 DCR 3582 (March 15, 2013).
