District of Columbia Municipal Regulations


406
WATER QUALITY ─ CONTAMINATION
406.1
A swimming pool, spa pool, or sauna shall be deemed contaminated when one (1) of the following conditions exists:

(a)
More than one (1) ten milliliter (10 ml) portion of a sample shows a positive test for coliform organisms when multi-tube fermentation technique is used; or more than one (1) coliform per fifty milliliters (50 ml) when the membrane filter test is used; or

(b)
Two (2) consecutive samples show a positive test for coliform organisms in any ten milliliter (10 ml) portion of a sample when the multi-tube fermentation technique is used or more than one (1) coliform per fifty milliliters (50 ml) when the membrane filter test is used; or 

(c)
Two (2) of any ten (10) consecutive samples show a positive test for coliform organisms in any of the ten milliliter (10 ml) portions of a sample when the multi-tube fermentation technique is used or more than one (1) coliform per fifty milliliters (50 ml) when the membrane filter test is used; or

(d)
When performing diarrheal/Cryptosporidium decontamination in aquatic venues, the maximum allowable cyanuric acid concentration shall be 15 ppm.

SOURCE: Final Rulemaking published at 64 DCR 5359 (June 9, 2017).
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