District of Columbia Municipal Regulations


407
RECIRCULATION AND TREATMENT SYSTEM ─ CROSS-CONNECTION PREVENTION
407.1
An atmospheric break or approved back flow prevention device shall be provided in each pool water supply line that is connected to a public water supply. 

407.2
Vacuum breakers shall be installed on all hose bibbs.

SOURCE: Final Rulemaking published at 64 DCR 5359 (June 9, 2017).
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