District of Columbia Municipal Regulations


403
HIGH-RISE BUILDINGS

Strike Section 403.3.2, Water supply to required fire pumps, of the International Building Code in its entirety without substitution.

Strike Section 403.4.5 of the International Building Code in its entirety and insert new Section 403.4.5 in the Building Code in its place to read as follows:

403.4.5 Emergency responder radio coverage. Emergency responder radio coverage shall be provided in accordance with Section 510 of the Fire Code.

Strike Section 403.5.1, Remoteness of interior exit stairways, of the International Building Code in its entirety without substitution.

Strike Section 403.6.1, Fire service access elevator, of the International Building Code in its entirety without substitution.

SOURCE: Final Rulemaking published at 61 DCR 2782 (March 28, 2014 – Part 2); as amended by Final Rulemaking published at 62 DCR 103 (January 2, 2015).
The District of Columbia Building Code (2013), referred to as the “Building Code,” consists of the 2012 edition of the International Building Code as amended by the District of Columbia Building Code Supplement (2013)(12  DCMR A). The International Building Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/ibc/2012/index.htm?bu=IC-P-2012-000001&bu2=IC-P-2012-000019.
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