District of Columbia Municipal Regulations


604 
ELECTRICAL FACILITIES

Strike Section 604.2 of the International Property Maintenance Code in its entirety and insert new Section 604.2 in the Property Maintenance Code in its place to read as follows:

604.2 
Service.  
The size and usage of appliances and equipment shall serve as a basis for determining the need for additional facilities in accordance with NFPA 70.  Dwelling units shall be served by a three-wire, 120/240 volt, single-phase electrical service having a rating of not less than 60 amperes.

Exception:  For installations consisting of not more than two 2-wire branch circuits, service disconnecting means shall have a rating of not less than 30 amperes.

SOURCE: Final Rulemaking published at 61 DCR 3196 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Property Maintenance Code (2013), referred to as the “Property Maintenance Code,” consists of the 2012 edition of the International Property Maintenance Code, published by the International Code Council (ICC), as amended by the District of Columbia Property Maintenance Code Supplement (2013) (12 DCMR G). The International Property Maintenance Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/ipmc/2012/index.htm?bu=IC-P-2012-000006&bu2=IC-P-2012-000019. 
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