1518
LOT OCCUPANCY, IMPERVIOUS SURFACE, AND SIDE YARD RESTRICTIONS (FH/TSP)

1518.1
The principal building and any accessory building on the lot shall not exceed total lot occupancy of thirty percent (30%).

1518.2
The maximum impervious surface coverage on a lot shall be fifty percent (50%); provided this subsection shall not:

(a)
Preclude enlargement of a principal building in existence as the effective date of the FH/TSP overlay; or

(b)
Create nonconformity of a structure as regulated by Chapter 20 of this title.

1518.3
To the extent a side yard is required in the underlying zone district, the minimum side yard requirement for all buildings, accessory buildings, or additions to buildings shall be twenty-four (24) feet in the aggregate, with no single side yard having a width of less than eight (8) feet.


SOURCE: Final Rulemaking published at 54 DCR 4835, 4841 (May 18, 2007).

