District of Columbia Municipal Regulations


503 
GENERAL BUILDING HEIGHT AND AREA LIMITATIONS
Strike Section 503.1.1 of the International Building Code in its entirety and insert new Section 503.1.1 in the Building Code in its place to read as follows:
503.1.1 Special industrial occupancies.  Buildings and structures designed to house low-hazard industrial processes that require large areas and unusual heights to accommodate craneways or special machinery and equipment, including among others, rolling mills; structural metal fabrication shops and foundries; or collection and treatment of sewage and stormwater, or the production and distribution of electric, gas, water or steam power, shall be exempt from the height and area limitations of Table 503.  Ordinary repairs of such buildings or structures shall include specifically engineered structural and mechanical components designed for removal and replacement in kind.
Strike Groups B, M, S-1 and S-2 in Table 503 of the International Building Code, in their entirety and insert new Groups B, M, S-1 and S-2 in their place in Table 503 of the Building Code to read as follows: 
TABLE 503 ALLOWABLE BUILDING HEIGHTS AND AREASa, b
Building height limitations shown in feet above grade plane. Story limitations shown as stories above grade plane. Building area limitations shown in square feet, as determined by the definition of “Area, building,” per story
	GROUP 
	
	TYPE OF CONSTRUCTION 

	
	
	TYPE I 
	TYPE II 
	TYPE III 
	TYPE IV 
	TYPE V 

	
	
	A 
	B 
	A 
	B 
	A 
	B 
	HT 
	A 
	B 

	
	HEIGHT (feet) 
	UL 
	160 
	65 
	55 
	65 
	55 
	65 
	50 
	40 

	
	STORIES(S) 
AREA (A) 

	B 
	S 
A 
	UL 
UL 
	11 
UL 
	5 
37,500 
	4
23,000 
	5 
28,500 
	 4
19,000 
	5 
36,000 
	3 
18,000 
	2 
9,000 


	GROUP 
	
	TYPE OF CONSTRUCTION 

	
	
	TYPE I 
	TYPE II 
	TYPE III 
	TYPE IV 
	TYPE V 

	
	
	A 
	B 
	A 
	B 
	A 
	B 
	HT 
	A 
	B 

	
	HEIGHT (feet) 
	UL 
	160 
	65 
	55 
	65 
	55 
	65 
	50 
	40 

	
	STORIES(S) 
AREA (A) 

	M 
	S 
A 
	UL 
UL 
	11 
UL 
	4 
21,500 
	4
12,500 
	4 
18,500 
	 4
12,500 
	4 
20,500 
	3 
14,000 
	1 
9,000 

	S-1 
	S 
A 
	UL 
UL 
	11 
48,000 
	4 
26,000 
	 3
17,500 
	3 
26,000 
	3
17,500 
	4 
25,500 
	3 
14,000 
	1 
9,000 

	S-2 
	S 
A 
	UL 
UL 
	11 
79,000 
	5 
39,000 
	4 
26,000 
	4 
39,000 
	4 
26,000 
	5 
38,500 
	4 
21,000 
	2 
13,500 


SOURCE: Final Rulemaking published at 61 DCR 2782 (March 28, 2014 – Part 2).
The District of Columbia Building Code (2013), referred to as the “Building Code,” consists of the 2012 edition of the International Building Code as amended by the District of Columbia Building Code Supplement (2013)(12  DCMR A). The International Building Code is copyrighted by the International Code Council and therefore is not republished here. However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/ibc/2012/index.htm?bu=IC-P-2012-000001&bu2=IC-P-2012-000019.
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