District of Columbia Municipal Regulations


605
ELECTRICAL EQUIPMENT

Insert new Section 605.4 in the Property Maintenance Code to read as follows:

605.4 
Switchboards of 1000 amperes or larger.  Preventative maintenance shall be performed on switchboards having a capacity of 1000 amperes or larger as required by Article 408.23 of the Electrical Code, as amended.

SOURCE: Final Rulemaking published at 61 DCR 3196 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Property Maintenance Code (2013), referred to as the “Property Maintenance Code,” consists of the 2012 edition of the International Property Maintenance Code, published by the International Code Council (ICC), as amended by the District of Columbia Property Maintenance Code Supplement (2013) (12 DCMR G). The International Property Maintenance Code is copyrighted by the ICC and therefore is not republished here. However, a copy of the text may be obtained at: http://publicecodes.cyberregs.com/icod/ipmc/2012/index.htm?bu=IC-P-2012-000006&bu2=IC-P-2012-000019. 
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