District of Columbia Municipal Regulations


607
BUILDING SERVICE WATER HEATING SYSTEMS

Strike Section 607.2.2 of the International Green Construction Code in its entirety and insert new Section 607.2.2 in the Green Construction Code in its place to read as follows:

607.2.2 Water heater controls for dwelling units.  Water heaters installed in dwelling units in buildings shall be equipped with external water temperature thermostat controls.

Strike Section 607.3 of the International Green Construction Code in its entirety without substitution.
Strike Section 607.4 of the International Green Construction Code in its entirety without substitution.
Strike Section 607.5 of the International Green Construction Code in its entirety without substitution.

Strike Section 607.6 of the International Green Construction Code in its entirety without substitution.

Strike Section 607.7 of the International Green Construction Code in its entirety without substitution.

SOURCE: Final Rulemaking published at 61 DCR 3356 (March 28, 2014 – Part 2); as corrected by Errata Notice published at 61 DCR 5246 (May 23, 2014).

The District of Columbia Green Construction Code (2013) , referred to as the “Green Construction Code,” consists of the 2012 edition of the International Green Construction Code published by the International Code Council (ICC), as amended by the District of Columbia Green Construction Code Supplement (2013)(12 DCMR K).  The International Green Construction Code is copyrighted by the International Code Council and therefore is not republished here.  However, a copy of the text may be obtained at:
http://publicecodes.cyberregs.com/icod/igcc/2012/index.htm?bu=IC-P-2012-000023&bu2=IC-P-2012-000019. 
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