1306
MAXIMUM PERMISSIBLE OCCUPANCY OF HOTEL AND MOTEL ROOMS

1306.1
Each room used for sleeping purposes by not more than two (2) transients shall be a habitable room containing at least seventy square feet (70 ft.2) of habitable room area.

1306.2
Each room used for sleeping purposes by three (3) or more transients shall be a habitable room containing at least thirty square feet (30 ft.2) of habitable room area for each occupant of the room.


SOURCE: The Housing Regulations of the District of Columbia, 5G DCRR § 7301, Commissioners’ Order 53-1503 (August 11, 1955).

