6436
DRESSING AND SANITARY FACILITIES - SHOWER FACILITIES, NUMBERS, AND WATER TEMPERATURE*

6436.1
A swimming pool or spa shall have at a minimum the following number of shower facilities:

(a)
One (1) shower for female bathers;

(b)
One (1) shower for male bathers; and

(c)
A minimum of two (2) shower heads for each sex. A minimum of one (1) additional shower head shall be required for each sex, and for each additional fifty (50) male or female bathers.

6436.2
Water temperature at the shower heads shall not exceed one hundred and ten degrees (110°F) (forty-three degrees Centigrade (43°C)).

6436.3
The water heater and thermostatically-controlled mixing valves shall be inaccessible to non-staff persons and shall be capable of providing two gallons per minute (2 gpm).


SOURCE: Final Rulemaking published at 55 DCR 012845 (December 26, 2008).

