District of Columbia Municipal Regulations


1003  
PERVIOUS SURFACE
1003.1
In the R-1A/CBUT zone, the minimum percentage of pervious surface of a lot, shall be fifty percent (50%), provided that this subsection shall not:

(a)
Preclude enlargement of a principal building in existence as of July 30, 1999; or

(b)
Create nonconformity of a structure as regulated by Subtitle C, Chapter 2.

SOURCE: Final Rulemaking published at 63 DCR 2447, 2834 (March 4, 2016 – Part 2); as amended by Final Rulemaking published at 63 DCR 10932 (August 26, 2016); as amended by Final Rulemaking published at 68 DCR 013834 (December 24, 2021); as amended by Final Rulemaking published at 70 DCR 011297 (August 25, 2023).
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