District of Columbia Municipal Regulations


1004

DENSITY
1004.1
In the NMU-4/CC2 zone, the maximum permitted floor area ratio (FAR) shall be as set forth in the following table:

TABLE H § 1004.1: MAXIMUM PERMITTED FLOOR AREA RATIO

	Zone
	Maximum Total FAR
	Maximum Non-Residential FAR 

	NMU-4/CC2 
	3.0

3.6 (IZ)
	1.5


1004.2
In the NMU-4/CC1 zone, new construction that preserves an existing façade constructed before 1958 is permitted an increase of 0.5 FAR to the maximum permitted density.

SOURCE: Final Rulemaking published at 72 DCR 007328 (June 27, 2025).
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